SECTION 09 06 05 – product and finish schedule

PRODUCT AND FINISH SCHEDULE USER’S GUIDE:

Item Codes always have two letters followed by two digits.   
Example: CL1 or CLG-1 is now CL01, This is done to enable the computer programs to correctly sort codes alpha-numerically.

* Always edit this document with hidden text visible. Hidden text can be identified by its dotted underline. Hidden text does not normally print in the final document.
* Copy and paste tables as required. Be sure to copy the empty line space (hard return = ¶) at the top of each table and paste it at the following empty line space. If tables become joined together they can be separated by cursoring on the first line of a table and from the Table Tools Layout ribbon click on “split table”.
* Remove the unused finish code tables that are not being used on your project and then remove the unused items by deleting the rows from the ‘Finish Code Index” table.
* Coordinate Item Code tables with the applicable Specification Section MasterFormat Numbers and Titles.
* Arrange the tables alpha-numerically by “Item Code.”
* If you need to create a new ‘Item Code’, be sure it has not already been assigned to represent something different. Refer to the master list of ‘Item Codes for Schedules’ used in all of Genlser’s Schedules by [clicking here](http://gportal/itsc/Shared%20Documents/20_Shared%20Documents/ITEM%20CODES/Item%20Codes%20for%20Schedules.xlsx).
* A completed Product and Finish Schedule should not have any bold [text] or <text> . Keystrokes Ctrl-A selects all text and Ctrl-B key toggles the text from bold to regular.

|  |  |  |
| --- | --- | --- |
|  | PRODUCT AND FINISH CODE INDEX |  |
| Item Code | Specification Section Title | Section Number |
| MT## | [Decorative Metal Finishes](#Decorative_Metal_1) | 05 70 00 |
| WD## | [Wood, Interior Architectural Woodwork](#Wood_1) (lumber & veneer) | 06 40 23 |
| WB## | [Wood Base, Interior Architectural Woodwork](#Wood_Base_1) | 06 40 23 |
| PL## | [Plastic Laminate, Interior Architectural Woodwork](#Plastic_Laminate_1) | 06 40 23 |
| UP## | [Upholstery, Interior Architectural Woodwork](#Upholstery_1) for *banquette seating* | 06 40 23 |
| GL## | [Glazing](#Glazing_1) | 08 80 00 |
| GF## | [Glazing Surface Films](#Glazing_Surface_Films_1); Decorative Films | 08 87 00 |
| TL## | [Tiling (Ceramic)](#Ceramic_Tiling_1) | 09 30 00 |
| TL## | [Tiling (Porcelain, Quarry, Paver, Glass, Metal)](#Tiling_1) | 09 30 00 |
| ST## | [Stone Tiling](#Stone_Tiling_1) *for stone less than ¾-inch thick, thick or thin-set* | 09 30 33 |
| CL## | [Acoustical Panel Ceilings](#Acoustical_Panel_Ceiling_1) *for panels 2- by 2-feet or larger and suspension grids* | 09 51 13 |
| CL## | [Suspended Wood Ceilings](#Suspended_Wood_Ceilings_1); Linear Wood Ceilings | 09 54 26 |
| FW## | [Fabric-Wrapped Ceiling Panels](#Fabric_Wrapped_Ceilings_1) | 09 54 43 |
| RT## | [Cork Flooring](#Cork_Flooring_1) | 09 62 29 |
| WF## | [Wood Flooring (Strip and Plank)](#Wood_Flooring_1) | 09 64 29 |
| RS## | [Resilient Sheet Flooring](#Resilient_Flooring_1) | 09 65 00 |
| RT## | [Resilient Tile Flooring](#Resilient_Flooring_2) (Rubber, VCT, Vinyl) | 09 65 00 |
| RT## | [Static-Control Resilient Flooring](#Static_Control_Resilient_Flooring_1) | 09 65 00 |
| RS## | [Linoleum Flooring](#Linoleum_Flooring_1) | 09 65 00 |
| RB## | [Resilient Wall Base and Accessories](#Resilient_Wall_Base_1) (Vinyl and Rubber) | 09 65 13 |
| CP## | [Tile Carpeting](#Tile_Carpenting_1) (Modular) | 09 68 13 |
| CP## | [Sheet Carpeting](#Sheet_Carpeting_1) (Broadloom) | 09 68 16 |
| AF## | [Access Flooring](#Access_Flooring_1) | 09 69 00 |
| WC## | [Wall Coverings](#Wall_Covering_1) | 09 72 00 |
| SF## | [Stretched-Fabric Wall Systems](#Stretched_Fabric_Wall_Systems_1) *for fabric applied on site-built frame, walls & ceilings* | 09 77 13 |
| FW## | [Fixed Fabric-Wrapped Panels](#Fixed_Fabric_Panels_1) | 09 77 23 |
| PT## | [Interior Painting](#Interior_Painting_1) *spec for both interior only* | 09 91 23 |
| PR## | [Impact Resistant Wall Coverings](#Impact_Resistant_Coverings_1) | 10 26 23 |
| CG## | [Corner Guards](#Corner_Guards_1) | 10 26 23 |
| SC## | [Stone Countertops](#Stone_Countertops_1) (Natural Stone) | 12 36 40 |
| SC## | [Simulated Stone Countertops](#Simulated_Stone_Countertops_1) (Quartz Surfacing) | 12 36 61 |
| SS## | [Solid Surface Countertops](#Solid_Surface_Countertops_1) | 12 36 61.16 |
| WT## | [Curtains and Drapes](#Curtains_1) | 12 22 00 |
| WT## | [Roller Window Shades](#Roller_Windows_1) | 12 24 13 |
| AR## | [Area Rug](#Area_Rug_1) | 12 48 53 |

|  |  |  |
| --- | --- | --- |
| MT## | decorative metal | 05 70 00 |
| Item Code | Specification |
| Material / Alloy | [**Aluminum**] [**Bronze**] [**Brass**] [**Stainless Steel**] [**Steel and Iron**] | Insert IMAGE Here |
| Finish | Aluminum Finishes: [**Clear Anodized**] [**Colour Anodized**] [**Baked-Enamel**]  Bronze and Brass Finishes: **[Buffed Finish (smooth specular)**] [**Hand-Rubbed Finish, Lacquered with Clear, Organic Coating**] [**Statuary Conversion Coating over Satin Finish**] [**Patina Conversion Coating**] [**Statuary Conversion Coating, Bright Relieved and Lacquered with Clear, Organic Coating**] [**Blackened, Bright Relieved, and Lacquered with Clear, Organic Coating**]  Stainless Steel Finishes: **[Cold-Rolled, Unpolished Finish: No. 2B**] [**Directional Polish: No. 4**] [**Non-Directional Polish: No. 4**] [**Satin, Directional Polish: No. 6**] [**Satin, Reflective, Directional Polish: No. 7**] [Mirror**, Non-Directional Polish: No. 8**]  Steel and Iron Finishes: **[Galvanized**] [**Factory Primed**] [**Powder-Coated**] |
| Colour | [**Match sample**] <**Insert manufacturer and manufacturer’s designation**> |
| Location |  |
| Notes | Match architect’s sample |

|  |  |  |
| --- | --- | --- |
| WD## | Wood (Lumber and Veneer) | 06 40 23 |
| Item Code | interior architectural woodwork | Specification |
| Item | Wood [veneer] [and] [lumber] | Insert IMAGE Here |
| Supplier |  |
| Flitch Number |  |
| Species | [**Anigre**] [**American Black Cherry**] [**African Mahogany**] [**Select White Maple**] [**Red Oak**] [**White Oak**] [**Amerian Black Walnut**] <**Insert Species**> |
| Cut | [**Plain sawn or sliced**] [**Rift sawn or cut**] [**Quarter sawn or cut**] |
| Finish | [**Clear**] [**Match sample** from designer] [from client] |
| Sheen | [**Flat, 10-25**] [**Satin, 30-50**] [**Semigloss, 55-75**] [**Gloss, 80-100**] |
| Location |  |
| Notes | See specification section for matching requirements unless otherwise indicated on the Drawings  [book-matched] [slip-matched] |
| **CAN ULC S102**  **Certificate saved?** | * **Yes** * **No** |

|  |  |  |
| --- | --- | --- |
| WB## | Wood Base | 06 40 23 |
| Item Code | interior architectural woodwork | Specification |
| Item | Wood [**veneer**] [**lumber**] | Insert IMAGE Here |
| Supplier | **[N/A] <Insert Name>** |
| Flitch Number | **[N/A] <Insert Reserved Flitch Number>** |
| Species | **[MDF** for opaque**]** **[Solid hardwood** for opaque**]** [**Anigre**] [**American Black Cherry**] [**African Mahogany**] [**Select White Maple**] [**Red Oak**] [**White Oak**] [**Amerian Black Walnut**] <**Insert Species**> |
| Cut | **[N/A]** [**Plain sawn or sliced**] [**Rift sawn or cut**] [**Quarter sawn or cut**] |
| Finish | **[Opaque, Paint Colour P<#>]** [**Transparent, Clear**] **[Transparent, Stained]** [**Match Architect's sample**] |
| Sheen | [**Flat, 10-25**] [**Satin, 30-50**] [**Semigloss, 55-75**] [**Gloss, 80-100**] |
| Base Detail Key In |  |
| Contact |  |
| Notes |  |
| **CAN ULC S102**  **Certificate saved?** | * **Yes** * **No** |

|  |  |  |
| --- | --- | --- |
| PL## | Plastic laminate | 06 40 23 |
| Item Code | interior architectural woodwork | Specification |
| Item | Plastic Laminate, HDPL | Insert IMAGE Here |
| Manufacturer | [**Abet Laminati, Abet, Inc.**] [**Formica Corporation**] [**Nevamar; Div. of Panolam Industries.**] [**Laminart**] [**Pionite; Div. of Panolam Industries.**] [**Wilsonart International.**] <**Insert manufacturer.**> |
| Product Name |  |
| Product Number |  |
| Colour |  |
| Finish |  |
| Contact |  |
| Notes |  |

|  |  |  |
| --- | --- | --- |
| UP## | Upholstery | 06 40 23 |
| Item Code | interior architectural woodwork | Specification |
| Manufacturer |  | Insert IMAGE Here |
| Product Name |  |
| Product # |  |
| Colour |  |
| Finish |  |
| Contact |  |
| Notes | Finish – Nan-o-Tex, Gore; Applied acrylic backing, Fabric Direction - Railroad |

|  |  |  |
| --- | --- | --- |
| GL## | glazing | 08 80 00 |
| Item Code | Specification |
| Type | **[Standard Annealed]** **[Tempered]** **[Heat-Strengthened] [Laminated] [Insulated Glazing Unit]** | Insert IMAGE Here |
| Colour | **[Clear]** **[Low-Iron Ultra Clear] [Tinted] <Insert Colour>** |
| Thickness |  |
| Location |  |
| Notes |  |
| **GPS Standards v1.0 Tracking** | * **Yes** | **\*Note this applies to Decorative Glazing only** |

|  |  |  |
| --- | --- | --- |
| GF## | glazing surface films | 08 87 00 |
| Item Code | Specification |
| Manufacturer |  | Insert IMAGE Here |
| Product Name |  |
| Product Number |  |
| Colour |  |
| Finish |  |
| Location |  |
| Notes |  |

|  |  |  |
| --- | --- | --- |
| TL## | Ceramic | 09 30 00 |
| Item Code | tiling | Specification |
| Manufacturer | [**American Marazzi Tile, Inc.**] [**American Olean; Div. of Dal-Tile International Corp.**] [**Buchtal Corporation USA**] [**Cerim-Floor Gres Ceramiche**] [**Crossville Ceramics Company, L.P.**] [**Daltile; Div. of Dal-Tile International Inc.**] [**Florida Tile Industries, Inc.**] [**GranitiFiandre**] [**Interceramic**] [**KPT, Inc.**] [**Laufen USA**] [**Lone Star Ceramics Company**] [**Metropolitan Ceramics**] [**Monarch Tile, Inc.**] [**Porcelanite, Inc.**] [**Quarry Tile Company**] [**Seneca Tiles, Inc.**] [**Summitville Tiles, Inc.**] [**United States Ceramic Tile Company**] [**Winburn Tile Manufacturing Company**] | Insert IMAGE Here |
| Product Name |  |
| Product Number |  |
| Colour |  |
| Size | [Ceramic Mosaics: **1 by 1 inch**] [**1 by 2 inches**] [**2 by 2 inches**]  Ceramic Wall Tiles: [**4-1/4 by 4-1/4 inches**] [**3 by 6 inches**] [**6 by 4-1/4 inches**] [**6 by 6 inches**] [200 by 200 mm] [250 by 250 mm] [200 by 300 mm] <***Insert size***> |
| Finish | Ceramic Mosaic, Wall, Quarry and Paver Tiles: [**Unglazed**] [**Bright, opaque**] [**Mat, opaque**] [**Semimat, opaque**] [**Vellum, opaque**] [**Crystalline**] <***Insert glaze description***>  Unglazed Quarry Tiles: [**Nonabrasive, smooth**] [**Nonabrasive, textured**] [**Abrasive aggregate embedded in surface**] |
| Grout Mfr. | **[Custom Building Products] [Laticrete International, Inc.]** **[Mapei Corporation]** |
| Grout Colour |  |
| Grout Type | **[Type 1] [Type 2] [Type 3] [Type 4];** refer to specifications on grout type. |
| Joint width | **[1/16-inch]** **[1/8-inch]** **[1/4-inch]** **[3/8-inch]** **[1/2-inch]** |
| Joint Sealant Mfr | **[n/a] <insert>** |
| Jt. Sealant Colour | **<insert>** |
| Tile Base Edge | **Top edge: [Square]** **[bullnosed];**  **Bottom edge: [square] [coved]** |
| Tile Base Corner | **Internal corner: [Square lapped]** **[square mitred] [coved]**  **External corner: [Square lapped]** **[square mitred] [coved]** |
| Base Detail Key |  |
| Location |  |
| Notes |  |

|  |  |  |
| --- | --- | --- |
| TL## | Porcelain Quarry, Glass, Metal | 09 30 00 |
| Item Code | tiling | Specification |
| Manufacturer | [**American Marazzi Tile, Inc.**] [**American Olean; Div. of Dal-Tile International Corp.**] [**Buchtal Corporation USA**] [**Cerim-Floor Gres Ceramiche**] [**Crossville Ceramics Company, L.P.**] [**Daltile; Div. of Dal-Tile International Inc.**] [**Florida Tile Industries, Inc.**] [**GranitiFiandre**] [**Interceramic**] [**KPT, Inc.**] [**Laufen USA**] [**Lone Star Ceramics Company**] [**Metropolitan Ceramics**] [**Monarch Tile, Inc.**] [**Porcelanite, Inc.**] [**Quarry Tile Company**] [**Seneca Tiles, Inc.**] [**Summitville Tiles, Inc.**] [**United States Ceramic Tile Company**] [**Winburn Tile Manufacturing Company**] | Insert IMAGE Here |
| Product Name |  |
| Product Number |  |
| Colour |  |
| Size | Glazed Wall Tiles: [**4-1/4 by 4-1/4 inches**] [**3 by 6 inches**] [**6 by 4-1/4 inches**] [**6 by 6 inches**] [200 by 200 mm] [250 by 250 mm] [200 by 300 mm] <***Insert size***>  Quarry Tiles: [**3 by 3 inches**] [**4 by 4 inches**] [**6 by 3 inches**] [**6 by 6 inches**] [**8 by 3-7/8 inches**] [**7-5/8 by 7-5/8 inches**] [**8 by 8 inches**] [160 by 320 mm] [140 by 280 mm] [300 by 300 mm] <***Insert size***>  Paver Tiles: [**7-3/4 by 3-7/8 inches**] [**7-7/8 by 7-7/8 inches**] [**11-13/16 by 11-13/16 inches**] [**200 by 200 mm**] [**300 by 300 mm**] <***Insert size***> |
| Finish | Wall, Quarry and Paver Tiles: [**Unglazed**] [**Bright, opaque**] [**Mat, opaque**] [**Semimat, opaque**] [**Vellum, opaque**] [**Crystalline**] <***Insert glaze description***>  Unglazed Quarry Tiles: [**Nonabrasive, smooth**] [**Nonabrasive, textured**] [**Abrasive aggregate embedded in surface**] |
| Grout Mfr. | **[Custom Building Products] [Laticrete International, Inc.]** **[Mapei Corporation]** |
| Grout Colour |  |
| Grout Type | **[Type 1] [Type 2] [Type 3] [Type 4];** refer to specifications on grout type. |
| Joint width | **[1/16-inch]** **[1/8-inch]** **[1/4-inch]** **[3/8-inch]** **[1/2-inch]** |
| Joint Sealant Mfr | **[n/a] <insert>** |
| Jt. Sealant Colour | **<insert>** |
| Tile Base Edge | **Top edge: [Square]** **[bullnosed];**  **Bottom edge: [square] [coved]** |
| Tile Base Corner | **Internal corner: [Square lapped]** **[square mitred] [coved]**  **External corner: [Square lapped]** **[square mitred] [coved]** |
| Base Detail Key |  |
| Location |  |
| Notes |  |

|  |  |  |
| --- | --- | --- |
| ST## | stone tiling | 09 30 33 |
| Item Code | Specification |
| Type | **[Granite] [Limestone] [Marble] [Quartz-Based Stone] [Serpentine] [Slate] [Travertine]** | Insert IMAGE Here |
| Source |  |
| Stone Name |  |
| Finish | Granite: [**Polished**] [**Honed**] [**Thermal**]  Limestone: [**Smooth**] [**Sand rubbed**] [**Plucked**] [**Sandblast textured (tapestry finish)**] [**Heavy sandblast textured (travertine finish)**]  Marble: [**Polished**] [**Honed**]  Quartz-Based Stone: [**Sand rubbed**] [**Natural cleft**] [**Thermal**]  Travertine: [**Polished**] [**Honed**]  Serpentine: [**Polished**] [**Honed**]  Slate: [**Honed**] [**Sand rubbed**] [**Natural cleft**] |
| Cut only applies to Travertine, some Limestones, some Marbles: | **[Fleuri (Vein)] [Cross]** cut |
| Contact |  |
| Notes |  |

|  |  |  |
| --- | --- | --- |
| CL## | aCoustical Panel Ceilings | 09 51 13 |
| Item Code | Specification |
| Manufacturer | **[Armstrong World Industries, Inc.]** **[USG Corporation]** **[BPB Celotex]** **[Decoustics]** **[Ecophon Certainteed, Inc.]** **[Tectum, Inc.] <Insert Manufacturer>** | Insert IMAGE Here |
| Product Name |  |
| Product Number |  |
| Colour | **[White]** **<insert custom Colour>** |
| Backing | **[none] [foil-backed]** |
| Size | **[24 by 24]** **[24 by 48]** **[30 by 30]** **<insert>** -inches |
| Thickness | **[3/4”] [1”] [1.5”]** |
| Panel Edge | **[Square] [Reveal sized to fit flange of exposed suspension system members] <*Insert manufacturer's special proprietary edge name*>** |
| Grid System | **[15/16 Tee]** **[9/16 Tee]** **[Bolt-slot with [1/8] [1/4]-inch reveal]** **[Extruded Screw-slot]** |
| Edge Trim | **[Angle]** **[Shadowline]** **[Fascia] <*Insert manufacturer’s special proprietary edge trim name*>** |
| Contact |  |
| Notes |  |
| CAN ULC S102  Certificate saved? | * Yes * No |
| GPS Standards v1.0 Tracking | * Yes |

|  |  |  |
| --- | --- | --- |
| CL## | suspenden wood ceilings | 09 54 26 |
| Item Code | Specification |
| Manufacturer | **[Armstrong World Industries, Inc.]** **[USG Corporation]** **[BPB Celotex]** **[Decoustics]** **[Ecophon Certainteed, Inc.]** **[Tectum, Inc.] <Insert Manufacturer>** | Insert IMAGE Here |
| Product Name |  |
| Product Number |  |
| Contact |  |
| Notes |  |

|  |  |  |
| --- | --- | --- |
| FW## | fabric-wrapped ceiling panels | 09 55 43 |
| Item Code | Specification |
| Manufacturer | **[Basis of design: Sound Concepts Canada Inc.] [Insert sole source manufacturer]** | Insert IMAGE Here |
| Product Name |  |
| Type | **[Acoustical]** **[Tackable]** **[Acoustical/Tackable]** |
| Panel Construction: | **[laminated to front face, edges, and back edge border of core] [stretched over front face of edge-framed core and bonded or attached to edges and back of frame] [insert description].** |
| Installation method: |  |
| Core Type | **[Glass-Fiberboard] [Glass-Fiber Blanket] [Medium-Density Fiberboard] [Medium-Density Fiberboard] [Particleboard].** |
| Core Face Layer | *Retain the following if different face layer is required for the core material to make the panels impact resistant, tackable or both*  [**tackable, impact-resistant, high-density board**] [**impact-resistant, acoustically transparent, copolymer sheet**] [**cork**]. |
| Core thickness | **[19] [25] [38] [51] mm overall** |
| Core overlay | *Retain the following if the design is tryingto achieve a “puffy” or “cushion” look.* Polyester batting [**13 mm** thick] [**manufacturer's standard thickness**] [**insert dimension**] |
| Edge Construction | *The following is the most common edge construction and used with glass and mineral fibre board boards.*  [**chemically hardened core with no frame**]  *Metal, PVC, and wood framed options are also available but may be less desireable for suspended panels in seismic areas.* [**extruded-aluminum or zinc-coated, rolled-steel frame**] [**extruded PVC frame**] [**wood frame, rabbeted, and splined with glued joints and machined corners**] [**insert requirement**]. |
| Edge Profile | [**Long edges kerfed and rabbeted to receive splines**] [**Chamfered (beveled)**] [**Eased (small radius)**] [**Mitered (beveled to a point)**] [**Radiused (bullnosed)**] [**Square**] [**Custom profile as indicated**] [**insert profile**]. |
| Corner Profile in elevation | [**Square**] [**Round, radius as indicated**] [**Custom as indicated**] [**insert description**] with continuous edge profile indicated |
| Panel joints | **[Butt Joint] [Recessed reveal] [Flush reveal] [Projecting reveal] [indicate dimensions][dimensions as indicated in the Drawings][as selected by Consultant from manufacturer's standard range].** |
| Facing material | **[Insert fabric specifications: Fabric manufacturer, Fabric No./Colour, Fabric roll width]** with [**Stain resistance**] [**Polymer flame resistance**] [**Acrylic backing, single coat**] [**Acrylic backing, double coat**] [**Latex backing**] [**Foam backing**] [**Knit backing**] [**insert other treatment**]. |
| Location |  |
| Notes |  |
| **CAN ULC S102**  **Certificate saved?** | * **Yes** * **No** |

|  |  |  |
| --- | --- | --- |
| RT## | Cork flooring | 09 62 29 |
| Item Code | Specification |
| Type | [natural core floor tile] [engineered cork-floor tile] [cork floating floor system] | Insert IMAGE Here |
| Manufacturer |  |
| Product Name |  |
| Product Number |  |
| Colour |  |
| Pattern | [Match Consultant's sample] [insert pattern]. |
| Size | **Tile: size**: [**305 x 305**] [**305 x 610**] [**610 x 610**] mm  **Plank size**: 900 x 305 mm. |
| Nominal Density | 1. **Tile density:** [Manufacturer's standard] [480] [544] [592] kg/ m3 minimum. 2. **Plank density:** 3. 1. Cork Top Layer: [448 kg/ m3] [Manufacturer's standard density] [insert density]. 4. 2. Interlocking Medium-Density Fiberboard Core: [720 kg/m3] [Manufacturer's standard density] [insert density]. 5. 3. Cork Underlayment Layer: [208 kg/m3] [Manufacturer's standard density] [insert density]. |
| Thickness | **Tile Thickness**: [4.0] [4.8] [8.0] mm.   1. **Plank Thickness:** 2. 1.Cork Top Layer: [3.2 mm] [Manufacturer's standard thickness] [insert thickness]. 3. 2.Interlocking Medium-Density Fiberboard Core: [6.3 mm] [Manufacturer's standard density] [insert thickness]. 4. 3.Cork Underlayment Layer: [2.0 mm] [Manufacturer's standard density] [insert thickness]. |
| Factory Finish | Factory Finish: [**Sanded or unfinished**] [**Waxed**] [**Polyurethane**] [**Polyurethane containing UV inhibitors**] [**Acrylic**] [**Match Consultant's sample**]. |
| Edge | [Tile: square edge][Plank: Tongue-and-groove type.] |
| Location |  |
| Notes | [**caution: do not install in wet areas]** |

|  |  |  |
| --- | --- | --- |
| WF## | wood flooring (strip and plank) | 09 64 29 |
| Item Code | Specification |
| Manufacturer/ Supplier | **[Insert manufacturer]** | Insert IMAGE Here |
| Species | [R**ed oak**] [White Oak] [H**ard maple**] [Beech][Yellow birch][**Douglas fir**] [**Insert species and grade]**.**[and Forest Stewardship Council certified]** |
| Grade | **[Select][Select or Better][#1 Common][#2 Common]** grade to NLGA grading rules for Canadian Lumber |
| Cut | [**Plain sawn**] [**Quarter/rift sawn**] [**Edge grain**] [**Vertical grain**] [**Insert cut]** |
| Colour | Match Architect's sample. |
| Face Width | [**2-1/4 inches (57 mm)**] [**3-1/8 inches (79 mm)**] [**5-1/8 inches (130 mm)**] [**Insert face width**] |
| Thickness | [**3/4 inch (19 mm)**] [**25/32 inch (20 mm)**] [**Insert thickness]** |
| Lengths | [**Random-length strips complying with applicable grading rules**] [**Lengths required to form pattern indicated**] |
| Edges | [**Square**] [**Beveled (eased)** for factory finished only] **[Tongue and groove edges and matched ends]** |
| Finish | [**Field finished**] [**Factory finished with UV urethane in Colour selected**] |
| Location |  |
| Notes |  |
| **Has this product been evaluated and confirmed to meet Gensler wood flooring guidelines** | * **Yes** * **No** |  |

|  |  |  |
| --- | --- | --- |
| RS## | resilient sheet flooring | 09 65 00 |
| Item Code | Specification |
| Manufacturer | **[Altro Floors]** **[Armstrong World Industries, Inc.] [Azrock Commercial Flooring, DOMCO] [Congoleum Corporation] [Forbo Industries, Inc.] [Lonseal, Inc.] [Mannington Mills, Inc.] [Flexco (USA), Inc.] [Tarkett Inc.] [TOLI International]** <***Insert manufacturer's name***> | Insert IMAGE Here |
| Product Name |  |
| Product Number |  |
| Colour | [**insert colour**] [**As indicated**] [**As selected by Consultant from manufacturer’s standard range** |
| Type | **[Vinyl sheet without backing] [vinyl sheet with backing] [rubber sheet without backing][rubber sheet with backing][with integral flash cove base]** |
| Thickness | **[2.0mm] [3.0mm]** |
| Sheet backing | **[Inorganic**] [**Organic**]. |
| Finish | UV cured polyurethane. |
| Wearing Surface | [**Smooth**] [**Embossed**]. |
| Installation method |  |
| Joints | **[Butt joint] [Welded joint][Chemical Bonding Compound]** |
| Weld Colour | [**As selected by Consultant from manufacturer's full range to contrast with flooring**] [**Match flooring**] [**Insert Colour**]. |
| Location | Refer to Finish Plans |
| Notes | Refer to Section 09 65 13 Resilient Base and Accessories for associated wall base |
| **GPS Standards v1.1 Tracking** | * **Yes** |  |

|  |  |  |
| --- | --- | --- |
| RT## | resilient tile flooring | 09 65 00 |
| Item Code | Specification |
| Type | **[Vinyl Composition Tile (VCT)] [Solid Vinyl Tile] [Rubber Tile] [Resilient Terrazzo Tile]** | Insert IMAGE Here |
| Manufacturer | \*\*\*Danny needs designer to review the following\*\*\*  Solid vinyl floor tile: **[Amtico International Inc.] [Armstrong World Industries, Inc.]** **[Azrock Commercial Flooring, DOMCO] [Estrie, American Biltrite (Canada) Ltd.]** **[Marley Flexco (USA), Inc.]** **[Roppe Corporation] [TOLI International]** **[VPI, LLC, Floor Products Division]**  Rubber floor tile: **[AFCO-USA, American Floor Products Company, Inc.]**  **[Burke Mercer Flooring Products]** **[Dodge-Regupol Inc., distributed by Gerbert Limited]** **[Endura]** **[Estrie, American Biltrite (Canada) Ltd.]** **[Johnsonite]** **[Marley Flexco (USA), Inc.]** **[Mondo Rubber International, Inc.]** **[Musson, R. C. Rubber Co.]** **[Nora Rubber Flooring, Freudenberg Building Systems, Inc.]** **[Pirelli Rubber Flooring]** **[R.C.A. Rubber Company]** **[Roppe Corporation]**  **Vinyl composition tile VCT: [Armstrong World Industries, Inc.] [Azrock Commercial Flooring, DOMCO]** **[Congoleum Corporation]** **[Flextile, Ltd.]** **[Mannington Mills, Inc.]** **[Tarkett Inc.]** <***Insert manufacturer's name***> |
| Product Name |  |
| Product Number |  |
| Colour | [**insert colour**] [**As indicated**] [**As selected by Consultant from manufacturer’s standard range**]. |
| Size | [**305 x 305**] [**460 x 460**] [**610 x 610**] [**914 x 914**] [**76 x 914**] [**insert dimensions**] mm |
| Thickness | [**2.0**] [**2.5**] [**3.0**] [**3.2**] mm |
| Recycled  Content | [**Insert percentage**] % post-consumer content, [**insert percentage**] % pre-consumer content |
| Location |  |
| Notes |  |
| **GPS Standards v1.1 Tracking** | * **Yes** |  |

|  |  |  |
| --- | --- | --- |
| RS## | linoleum flooring | 09 65 00 |
| Item Code | Specification |
| Manufacturer | **[Armstrong World Industries, Inc.] [Flooring Group]** **[Forbo Industries, Inc.] [Johnsonite]** <***Insert manufacturer's name***> | Insert IMAGE Here |
| Product Name |  |
| Product Number |  |
| Colour |  |
| Thickness |  |
| Tile Size/ Roll Width |  |
| Location |  |
| Notes |  |

|  |  |  |
| --- | --- | --- |
| RT## | static-control resilient flooring | 09 65 00 |
| Item Code | Specification |
| Type | **[Solid vinyl floor tile] [Rubber floor tile] [Vinyl composition tile (VCT)][Cork Flooring]** | Insert IMAGE Here |
| Manufacturer | Solid vinyl floor tile: **[Amtico International Inc.] [Armstrong World Industries, Inc.]** **[Azrock Commercial Flooring, DOMCO] [Estrie, American Biltrite (Canada) Ltd.]** **[Marley Flexco (USA), Inc.]** **[Roppe Corporation] [TOLI International]** **[VPI, LLC, Floor Products Division]**  Rubber floor tile: **[AFCO-USA, American Floor Products Company, Inc.]**  **[Burke Mercer Flooring Products]** **[Dodge-Regupol Inc., distributed by Gerbert Limited]** **[Endura]** **[Estrie, American Biltrite (Canada) Ltd.]** **[Johnsonite]** **[Marley Flexco (USA), Inc.]** **[Mondo Rubber International, Inc.]** **[Musson, R. C. Rubber Co.]** **[Nora Rubber Flooring, Freudenberg Building Systems, Inc.]** **[Pirelli Rubber Flooring]** **[R.C.A. Rubber Company]** **[Roppe Corporation]**  **Vinyl composition tile VCT: [Armstrong World Industries, Inc.] [Azrock Commercial Flooring, DOMCO]** **[Congoleum Corporation]** **[Flextile, Ltd.]** **[Mannington Mills, Inc.]** **[Tarkett Inc.]** <***Insert manufacturer's name***> |
| Product Name |  |
| Product Number |  |
| Colour |  |
| Size |  |
| Thickness |  |
| Contact |  |
| Notes |  |

|  |  |  |
| --- | --- | --- |
| RB## | resilient wall base and accessories | 09 65 13 |
| Item Code | Specification |
| Manufacturer | Vinyl wall base (Type TV) and Rubber wall base thermoplastic (Type TP):  **[Armstrong World Industries, Inc.] [Burke Mercer Flooring Products] [Johnsonite] [Flexco (USA), Inc.] [Roppe Corporation]**  Rubber wall base thermoset (Type TS ☺): **[Allstate Rubber Corporation, Stoler Industries, Div.] [Burke Mercer Flooring Products][ Roppe Corporation]** | Insert IMAGE Here |
| Product Name |  |
| Product Number |  |
| Colour | [**insert colour**] [**As indicated**] [**As selected by Consultant from manufacturer’s standard range**]. |
| Height Size | [**2 1/2 inches**] [**4 inches**] [**6 inches**] |
| Thickness | [**2.0mm (3/16 inch)] [3.2mm (1/8 inch)] [manufacture standard thickness]** |
| Style | [**Coved base at resilient and hard flooring; Straight base at carpet**] |
| Lengths | [**Cut lengths 1220 mm long minimum**] [**Coils in manufacturer's standard length**]. |
| Outside Corners | [**Site formed**] [**Preformed**]. |
| Inside Corners | [**Site formed**] [**Preformed**]. |
| Location | Refer to Finish Plan |
| Notes |  |
| **GPS Standards v1.0 Tracking** | * **Yes** |

|  |  |  |
| --- | --- | --- |
| CP## | tile carpeting (mOdular) | 09 68 13 |
| Item Code | Specification |
| Manufacturer | **[Bentely Prince Street]** **[C&A – a division of Tandus]** **[InterfaceFlor Commerical] [Invision]**  **[Lees]** **[Milliken]** **[Shaw Contract Group] <Insert Manufacturer>** | Insert IMAGE Here |
| Product Name |  |
| Product Number |  |
| Colour |  |
| Size | **[18 by 18]** **[24 by 24]** **[36 by 36]**-inches |
| Thickness |  |
| Finish |  |
| Type | Woven: Tufted: **[Loop Pile]** **[Tip Shear]** **[Cut & Loop]** |
| Yarn Content |  |
| Pile Height |  |
| Gage/Pitch | Tufted/woven |
| Pile Density |  |
| Stitches/inch |  |
| Face Weight | <**Insert ##**> ounces per square yard |
| Total Weight | <**Insert ##**> ounces per square yard |
| Backing | [type] |
| Dye Method | **[Solution dyed]** **[Yarn dyed]** **[Piece dyed]** |
| Sustainability | **[recycled backing] [low VOC] [Leed]** |
| Location |  |
| Installation method | [Release adhesive] [ TacTile] |
| Installation pattern | [Ashlar] [Brick] [random] [quarter-turned] |
| Notes |  |
| CAN ULC S102  Certificate saved? | * Yes * No |
| GPS Standards v1.0 Tracking | * Yes |

|  |  |  |
| --- | --- | --- |
| CP## | sheet carpeting (broadloom) | 09 68 16 |
| Item Code | Specification |
| Manufacturer |  | Insert IMAGE Here |
| Product Name |  |
| Product Number |  |
| Color |  |
| Construction | **[Woven] [Tufted]** |
| Type |  |
| Yarn Content |  |
| Pile Height | **[Woven] [Tufted]** |
| Gage/Pitch |  |
| Pile Density |  |
| Stitches/inch |  |
| Face Weight | <**Insert ##**> ounces per square yard |
| Total Weight | <**Insert ##**> ounces per square yard |
| Backing |  |
| Dye Method | **[Solution dyed]** **[Yarn dyed]** **[Piece dyed]** |
| Cushion |  |
| Contact |  |
| Notes |  |
| CAN ULC S102  Certificate saved? | * Yes * No |  |
| GPS Standards v1.0 Tracking | * Yes |  |

|  |  |  |
| --- | --- | --- |
| AF## | access flooring | 09 69 00 |
| Item Code | Specification |
| Manufacturer |  | Insert IMAGE Here |
| Product Name |  |
| Product Number |  |
| Color |  |
| Size |  |
| Finish |  |
| Contact |  |
| Notes |  |

|  |  |  |
| --- | --- | --- |
| WC## | wall coverings | 09 72 00 |
| Item Code | Specification |
| Manufacturer | **[Innovations]** **[JM Lynne – a division of Designtex] [Koroseal Interior Products] [Knoll] [Maharam] [MDC] [Wolf Gordon]** | Insert IMAGE Here |
| Product Name |  |
| Product Number |  |
| Type | [**mildew-resistant**] [**peelable**] [**strippable**] |
| Category | [**I, Decorative Only**] [**II, Decorative with Medium Serviceability**] [**III, Decorative with High Serviceability**] [**IV, Type I, Commercial Serviceability**] [**V, Type II, Commercial Serviceability**] [**VI, Type III, Commercial Serviceability**].  *Category I: For decorative purposes only*  *Category II:Primary decorative, but with more washable and colourfastness*  *Category III:For medium use where abrasion and stain resistance, scrubbing ability and increased colourfastness are required*  *Category IV Type 1: For use where higher abrasion and stain resistance are required for heavy consumer and light commercial use.*  *Category V: Type II: For use when better wearing qualities are required, exposure to wear is greater than normal.*  *Category VI, Type III: For use in heavy traffic areas.* |
| Colour |  |
| Pattern/texture | **[Random] [insert horizontal and vertical dimensions of repeat].** |
| Roll Width | [**686**] [**1372**] [**insert roll width**]mm |
| Backing | **[Acrylic]**  **[Paper]**  **[Fabric: [Scrim] [Osnaburg] [Drill] [Nonwoven]; Content: [Cotton] [Polyester] [Polycotton] [Polyester cellulose] [insert fibre content.]]** |
| Finish | **Stain-Resistant Coating: [**insert coating manufacturer's name and product identification**].** |
| Location |  |
| Notes |  |
| **CAN ULC S102**  **Certificate saved?** | * **Yes** * **No** |

|  |  |  |
| --- | --- | --- |
| SF## | Stretched-fabric wall systems | 09 77 13 |
| Item Code | Specification |
| Panel Type | **[Acoustical]** **[Tackable]** **[Acoustical/Tackable]** | Insert IMAGE Here |
| Manufacturer |  |
| Product Name |  |
| Product Number |  |
| Frame system | **[Extruded PVC]** **[Extruded aluminum] [exposed][concealed]** |
| Frame Colour | **[black][Natural][White] [Custom prefinished]** |
| Frame thickness | **[13mm (1/2inch)] [19mm (3/4inch)] [38mm(1-1/2inch)] [50mm(2inches)]** |
| Frame |  |
| Edge Profile | Square |
| Corner Profile in elevation | [**Square**] [**Round, radius as indicated on Drawings**] [**Custom as indicated on Drawings**] [**insert description**] |
| Panel joint | **[Butt Joint] [Recessed reveal**] [**Flush reveal**] [**Projecting reveal] [indicate dimensions] [dimensions as indicated in the Drawings]** [**as selected by Consultant from manufacturer's standard range]** |
| Fabric Mfr. |  |
| Fabric Name/No./Colour |  |
| Fabric Width |  |
| Fabric Treatment | [fire rating] |
| Location |  |
| Notes |  |
| **CAN ULC S102**  **Certificate saved?** | * **Yes** * **No** |

|  |  |  |
| --- | --- | --- |
| FW## | fixed fabric-wrapped panels | 09 77 23 |
| Item Code | Specification |
| Manufacturer | **[Basis of design: Sound Concepts Canada Inc.] [Insert sole source manufacturer]** | Insert IMAGE Here |
| Product Name |  |
| Type | **[Acoustical]** **[Tackable]** **[Acoustical/Tackable]** |
| Panel Construction: | **[laminated to front face, edges, and back edge border of core] [stretched over front face of edge-framed core and bonded or attached to edges and back of frame] [insert description].** |
| Installation method |  |
| Core Type | **[Glass-Fiberboard] [Glass-Fiber Blanket] [Medium-Density Fiberboard] [Medium-Density Fiberboard] [Particleboard].** |
| Core Face Layer | *Retain the following if different face layer is required for the core material to make the panels impact resistant, tackable or both*  [**tackable, impact-resistant, high-density board**] [**impact-resistant, acoustically transparent, copolymer sheet**] [**cork**]. |
| Core thickness | **[19] [25] [38] [51] mm overall** |
| Core overlay | *Retain the following if the design is tryingto achieve a “puffy” or “cushion” look.* Polyester batting [**13 mm** thick] [**manufacturer's standard thickness**] [**insert dimension**] |
| Edge Construction | *The following is the most common edge construction and used with glass and mineral fibre board boards.*  [**chemically hardened core with no frame**]  *Metal, PVC, and wood framed options are also available but may be less desireable for suspended panels in seismic areas.* [**extruded-aluminum or zinc-coated, rolled-steel frame**] [**extruded PVC frame**] [**wood frame, rabbeted, and splined with glued joints and machined corners**] [**insert requirement**]. |
| Edge Profile | [**Long edges kerfed and rabbeted to receive splines**] [**Chamfered (beveled)**] [**Eased (small radius)**] [**Mitered (beveled to a point)**] [**Radiused (bullnosed)**] [**Square**] [**Custom profile as indicated**] [**insert profile**]. |
| Corner Profile in elevation | [**Square**] [**Round, radius as indicated**] [**Custom as indicated**] [**insert description**] with continuous edge profile indicated |
| Panel joints | **[Butt Joint] [Recessed reveal] [Flush reveal] [Projecting reveal] [indicate dimensions][dimensions as indicated in the Drawings][as selected by Consultant from manufacturer's standard range].** |
| Facing material | **[Insert fabric specifications: Fabric manufacturer, Fabric No./Colour, Fabric roll width]** with [**Stain resistance**] [**Polymer flame resistance**] [**Acrylic backing, single coat**] [**Acrylic backing, double coat**] [**Latex backing**] [**Foam backing**] [**Knit backing**] [**insert other treatment**]. |
| Location |  |
| Notes |  |
| **CAN ULC S102**  **Certificate saved?** | * **Yes** * **No** |

|  |  |  |
| --- | --- | --- |
| PT## | interior painting | 09 91 23 |
| Item Code | Specification |
| Manufacturer | **[Benjamin Moore] [Dulux] [PPG] [Pratt & Lambert] [Sherwin Williams] <Insert Manufacturer>** | Insert IMAGE Here |
| Type | Latex is water-based paint, Alkyd is solvent (oil) based paint  **[Latex Interior Standard] [Latex Interior Institutional] [Latex Interior High Performance Architectural] [Light Industrial Coating Interior] [Alkyd Interior Standard] [Alkyd Interior Quick Dry] [Textured Coating] [Dry Fall Latex] [Dry Fall Alkyd][Floor coating water based][Floor coating Solvent Based][Floor coating Enamel Alkyd][Laqured]** |
| Colour Number |  |
| Colour Name |  |
| Sheen | This overrides the specification of flat on soffits & ceilings; Semi-gloss on wood & metal trim and doors **[Flat] [Satin][Eggshell] [Pearl]** **[Semi-Gloss]** **[Gloss]** |
| Location |  |
| Notes | PT-1: All areas unless otherwise noted. Include perimeter bulkheads, kneewalls, radiator covers, as applicable. |
| **GPS Standards v1.0 Tracking** | * **Yes** |

|  |  |  |
| --- | --- | --- |
| PR## | impact resistant wall coverings | 10 26 23 |
| Item Code | Specification |
| Manufacturer |  | Insert IMAGE Here |
| Product Name |  |
| Product Number |  |
| Colour |  |
| Finish |  |
| Contact |  |
| Notes |  |

|  |  |  |
| --- | --- | --- |
| CG## | corner guards | 10 26 23 |
| Item Code | Specification |
| Manufacturer |  | Insert IMAGE Here |
| Product Name |  |
| Product Number |  |
| Colour |  |
| Finish |  |
| Contact |  |
| Notes |  |

|  |  |  |
| --- | --- | --- |
| SC## | stone countertops | 12 36 40 |
| Item Code | Specification |
| Type | Natural Stone | Insert IMAGE Here |
| Variety | Natural Stone: **[Granite] [Limestone] [Marble] [Slate]** |
| Source |  |
| Manufacturer |  |
| Stone Name |  |
| Description | Granite: [**Uniform fine grained**] [**Uniform medium grained**], **[white][pink][gray][black][insert colour],[without veining][with veining**].  Marble: [**Uniform fine-to-medium grained], [white][insert colour],[with only slight veining]**  Serpentine: **[Match sample]**  Slate: **[Black][Blue-black] [Gray][Blue gray][Green][Red][with fine, even grain colour][match sample]** |
| Cut | Granite: [**Vein][Fleuri**][match sample]  Marble: [**Vein][Fleuri**][match sample]  Serpentine: **[match sample]**  Slate: **[match sample]** |
| Finish | Granite: [**Polished**] [**Honed**] [**Thermal][match sample**].  Marble: [**Polished**] [**Honed**][match sample]  Serpentine:  Slate: [**Honed**] [**Sand rubbed**] [**Natural cleft**] |
| Location |  |
| Notes | Cut natural stone from contiguous, matched slabs in which natural markings occur |

|  |  |  |
| --- | --- | --- |
| SC## | simulated stone countertops | 12 36 61 |
| Item Code | Specification |
| Type | Simulated Stone | Insert IMAGE Here |
| Variety | **[Quartz-Based Stone] [Cultured marble][Solid surface]** |
| Manufacturer | Cultured Marble: **[insert manufacturer name]**,  Quartz: **[Cambria]**, **[Zodiaq]**, **[Silestone]**, **[Icestone]**,, **[Caesarstone]**, **[Viatera]**, **[FormicaStone]** |
| Product Name |  |
| Product Number |  |
| Thickness |  |
| Colour |  |
| Finish | Quartz-Based Stone: [**Sand rubbed**] [**Natural cleft**] [**Thermal**] |
| Location |  |
| Notes |  |

|  |  |  |
| --- | --- | --- |
| SS## | solid surface countertops | 12 36 61.16 |
| Item Code | Specification |
| Manufacturer | [**DuPont Polymers; Corian**] **[Formica Corporation]** [**Wilsonart International, Div. of [Meganite Inc] [Samsung Chemical] [Corian DuPont]** | Insert IMAGE Here |
| Product Name |  |
| Product Number |  |
| Type | **[Standard Type Solid Surface] [Veneer Type Solid Surface]** |
| Colour | [**Insert Colour name and/or number**] |
| Thickness |  |
| Finish |  |
| Location |  |
| Notes |  |

|  |  |  |
| --- | --- | --- |
| WT## | curtains and drapes | 12 22 00 |
| Item Code | Specification |
| Fabric  Manufacturer |  | Insert IMAGE Here |
| Product Name |  |
| Product Number |  |
| Colour |  |
| Fiber Content |  |
| Width |  |
| Pattern Repeat Distance | <**Insert vertical distance**> vertically; <**Insert horizontal distance**> horizontally |
| Textile Treatments | [**Stain repellent**] [**Flame retardant, polymer type**] [**Stain repellent; and flame retardant, polymer type**] <**Insert requirements**> |
| Orientation | Run right [up the bolt] |
| Contact |  |
| Track |  |
| Pleating |  |
| Hems |  |
| Cords | [one side] [bi-parting] spring, weighted [sling rods] |
|  |  |
| Notes |  |
| **CAN ULC S109**  **Certificate saved?** | * **Yes** * **No** |

|  |  |  |
| --- | --- | --- |
| WT## | roller windows shades | 12 24 13 |
| Item Code | Specification |
| Product Name | **[MechoShade Thermoveil] [DFB Sales, Inc., Sol-R-Control] [Phifer SheerWeave] [Lutron] <Insert name>** | Insert IMAGE Here |
| No. / Series | **<Insert item number>** |
| Openness Factor | **[Opaque]** **[3%]** **[5%]** **[10%]** **[20%] <insert number>** |
| Colour | **<Insert Colour name>** |
| Contact |  |
| Notes |  |
| Product Name | **[MechoShade Thermoveil] [DFB Sales, Inc., Sol-R-Control] [Phifer SheerWeave] [Lutron] <Insert name>** |

|  |  |  |
| --- | --- | --- |
| AR## | area RUg | 12 48 53 |
| Item Code | Specification |
| Manufacturer |  | Insert IMAGE Here |
| Product Name |  |
| Product Number |  |
| Color |  |
| Size |  |
| Finish |  |
| Contact |  |
| Notes |  |

|  |  |  |
| --- | --- | --- |
| AR## | area RUg | 12 48 53 |
| Item Code | Specification |
| Manufacturer |  | Insert IMAGE Here |
| Product Name |  |
| Product Number |  |
| Colour |  |
| Size |  |
| Thickness |  |
| Cut |  |
| Species |  |
| Material / Alloy |  |
| Finish |  |
| Contact |  |
| Notes |  |
| **CAN ULC S102**  **Certificate saved?** | * **Yes** * **No** |

END OF SECTION