SECTION  – area rugs

1. GENERAL
   1. summary
      1. Section includes custom, hand-knotted rugs.
   2. related requirements
      1. Section 03 35 00: Concrete Finishing.
      2. Section 09 06 05: Product and Finish Schedule.
      3. Section 09 64 00: Wood Flooring.
      4. Section 09 65 00: Resilient Flooring and Accessories.
      5. Section 09 68 13: Tile Carpeting.
      6. Section 09 68 16: Sheet Carpeting.
      7. Section 09 69 00: Access Flooring.
   3. reference STANDARDS
      1. Except as modified by governing codes and by the Contract Documents, comply with the applicable provisions and recommendations of the following:
         1. The Carpet and Rug Institute "The Carpet Specifiers' Handbook."
      2. The Carpet and Rug Institute "CRI 104 Standard for Installation of Commercial Carpet, edition Sept. 2015."
   4. submittals
      1. Product Data: For each product indicated.
      2. Shop Drawings:
         1. Seam locations.
         2. Pattern type, repeat, location, direction, and starting point.
         3. Pile direction.
         4. Insets and borders.
      3. Samples: For each for each rug and exposed accessory and for each colour and pattern required.
   5. quality assurance
      1. Installer Qualifications: A qualified installer who is certified by the Floor Covering Installation Board or who can demonstrate compliance with its certification program requirements.
   6. DELIVERY, STORAGE, AND HANDLING
      1. Comply with CRI 104.
   7. FIELD CONDITIONS
      1. Comply with CRI 104.
      2. Environmental Limitations: Do not install rug until wet work in spaces is complete and dry, and ambient temperature and humidity conditions are maintained at the levels indicated for Project when occupied for its intended use.
   8. WARRANTY
      1. Rug Warranty: Manufacturer's standard form in which manufacturer agrees to replace rug that does not comply with requirements or that fails within 20 years from date of Substantial Completion. Warranty does not include deterioration or failure of rug from unusual traffic, failure of substrate, vandalism, or abuse. Failures include, but are not limited to, more than 10 percent loss of face fiber, edge raveling, snags, runs, and delamination.
2. Products
   1. AREA RUG (ARXX)
      1. Custom Area Rug: As indicated in Section 09 06 05 – Product and Finish Schedule.
3. Execution
   1. installation
      1. Install parallel to walls and borders.
      2. Provide protection until Substantial Completion.
      3. Install reducer strips to the adjacent floor finish.

end of section